**Royal Observatory Cape of Good Hope – 1916**

* January – wet thermometer reading, have an X above them. I have highlighted them in purple.
* February – 29 days (leap year).
* 21st of February – Vane out of adjustment
  + Direction gear taken down for repair, return on Feb 19.
* 24th of February – Vane again being adjusted.
* 29th of April – anemomter stopped (velocity).
* 17 to 20th of July – clock stopped working
* July 19th – clock taken down to be cleaned strated clock at 3:10, stopped again at 6:3- on July 20th
* July 20th – anemometer cleaned, set going at 2:45 pm
* 14th of August – snow on peak